### Bay Windows

Bay windows refer to raised windows not exceeding one structural bay width and cantilevered at least 0.5m high from the floor. Bay windows, except those approved before 1st January 2009, are included as GFA.

<https://www.ura.gov.sg/-/media/Corporate/Guidelines/Development-control/GFA/GFA-09B-Bay-windows_final.jpg?h=569&w=800>

*Bay Window (Section)*

*Last updated on 26 Jul 2023*