### Curtain Wall

For buildings with curtain walls fixed onto the main structure, the GFA is measured up to the middle of the outermost vertical facade element (e.g. the glass panel).



*Curtain Wall (Section)*



*Curtain Wall (Plan View)*