### Curtain Wall

For buildings with curtain walls fixed onto the main structure, the GFA is measured up to the middle of the outermost vertical facade element (e.g. the glass panel).

<https://www.ura.gov.sg/-/media/Corporate/Guidelines/Development-control/GFA/GFA-33A-Curtain-Wall.jpg?h=1000&w=1167>

*Curtain Wall (Section)*

<https://www.ura.gov.sg/-/media/Corporate/Guidelines/Development-control/GFA/GFA-33A-Curtain-Wall-Plan-View.jpg>

*Curtain Wall (Plan View)*

*Last updated on 8 Apr 2024*