### Service Ducts

Service ducts, including the thickness of the walls, are included as GFA once at the lowest floor, if the vertical shaft is entirely a void space.

If the service ducts are slabbed over at every floor, the service duct at each floor is included as GFA. Non- load bearing fire-stop material to compartmentalise the service ducts are excluded from GFA.

<https://www.ura.gov.sg/-/media/Corporate/Guidelines/Development-control/GFA/GFA-12C-Service-Duct-sectionlift-shaft--service-duct-section.jpg?h=503&w=800>

*Service Duct*

*Last updated on 26 Jul 2023*