### Access Points

Vehicular Access to Bungalow Plot

Only one vehicular access point shall be allowed per bungalow plot.



*Positioning vehicular access points*

The position of vehicular access point for bungalows shall consider roadside planting and kerbside parking space provision. Each plot's vehicular access point shall have a separation space of at least 6m from the neighbouring plot for a planting verge.

Entrance to a Landed House

Only one main entrance door for a single residential unit for family dwelling purposes shall be allowed in a landed house.

*Last updated on 5 July 2019*