### Catwalks

Unenclosed metal perforated catwalks meant for maintenance purposes and not exceeding 1.0m in width are excluded from GFA.

*Last updated on 5 Oct 2020*